Configurator Installation Instructions
1.OS Requirements: Windows 7 and above, MacOS 10.15 and above.
2.Package download Link for windows: https://y.gpstracktech.com/view/Configurator_windows_x86_64_latest.zip
 Package download Link for MacOS: https://y.gpstracktech.com/view/Configurator_darwin_universal_latest.zip
3.Installation Steps for Windows:
   3.1 After downloading the installer via step 2, right-click and run it as an administrator.
   3.2 Follow the instructions to select the installation directory for the program. Please ensure that there is at least 100MB of free space on the disk where the program will be installed.
   3.3 Upon completion of the installation, tick the "Run Configuration" box or double-click to open the application. At this point, when the device is connected, the program will automatically scan for the device's serial port and establish a connection with it.
4.Installation Steps for MacOS:
   4.1 Double-click the installer package "Configurator_universal.dmg". Follow the pop-up instructions to drag the installer package into the Applications folder.
   4.2 In the Applications folder, double-click the application to run it.

Note: When connecting the device for the first time, the system will automatically install the necessary drivers. Until the drivers are fully installed, the tool may not connect the device, which may result in a prolonged scanning period before a successful connection is established. This is normal behavior. Typically, wait for 2-3 minutes for the driver installation to complete.If the computer is blocked from the internet or the driver installation fails, please try manually loading the driver file (see file name: ft232r_usc_uard_river.zip)


Configurator安装说明
1.操作系统要求：Windows 7 and above，MacOS 10.15 and above.
2.Windows 下载地址：https://y.gpstracktech.com/view/Configurator_windows_x86_64_latest.zip
  MacOS下载地址：https://y.gpstracktech.com/view/Configurator_darwin_universal_latest.zip
3.windows系统安装步骤：
 3.1通过2下载安装包后，鼠标右键使用系统管理员身份运行。
 3.2根据指引选择程序安装目录等待安装，请确保程序所在磁盘剩余容量至少100MB。
 3.3安装完成后，勾选Run Configuration 或者双击打开应用，连接设备，程序将自动扫描设备串口并连接设备。
4.MacOS安装步骤
 4.1 双击安装包Configurator_universal.dmg后，按照弹窗指引将安装包拖动到application里。
 4.2 在application里双击应用运行。

注：首次连接设备，系统将会自动安装驱动程序，在驱动程序安装完成前，工具将无法识别设备，因此可能出现长时间扫描设备未能连接成功的情况，此为正常现象，通常等待2-3分钟驱动安装完成即可。若电脑禁网，或驱动安装失败，请尝试手动加载驱动文件（见文件名称:ft232r_usb_uart_driver.zip）






